3GPP TS 29.504 V15.2.0 (2018-12)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Core Network and Terminals;

5G System; Unified Data Repository Services;

Stage 3

(Release 15)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP..  
The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.  
Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices.

Keywords

3GPP, 5G System

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles - Sophia Antipolis

Valbonne - FRANCE

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2018, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 5

1 Scope 6

2 References 6

3 Definitions and abbreviations 7

3.1 Definitions 7

3.2 Abbreviations 7

4 Overview 7

5 Services offered by the UDR 8

5.1 Introduction 8

5.2 Nudr\_DataRepository Service 8

5.2.1 Service Description 8

5.2.1.1 Service and operation description 8

5.2.1.2 Service operation and data access authorization 8

5.2.2 Service Operations 9

5.2.2.1 Introduction 9

5.2.2.2 Query 9

5.2.2.2.1 General 9

5.2.2.2.2 Data retrieval 9

5.2.2.2.3 Retrieval of subset of a resource 10

5.2.2.3 Create 11

5.2.2.3.1 General 11

5.2.2.3.2 Data Creation using PUT 11

5.2.2.3.3 Data Creation using POST 12

5.2.2.4 Delete 12

5.2.2.4.1 General 12

5.2.2.4.2 Deleting Data 13

5.2.2.5 Update 13

5.2.2.5.1 General 13

5.2.2.5.2 Data Update using PATCH 13

5.2.2.5.3 Data Update using PUT 14

5.2.2.6 Subscribe 14

5.2.2.6.1 General 14

5.2.2.6.2 NF service consumer subscribes to notifications to UDR 14

5.2.2.6.3 Stateless UDM subscribes to notifications to UDR 15

5.2.2.7 Unsubscribe 16

5.2.2.7.1 General 16

5.2.2.7.2 Unsubscribe service operation 16

5.2.2.8 Notify 17

5.2.2.8.1 General 17

5.2.2.8.2 Notification to NF service consumer on data change 17

5.2.2.8.3 Notification to stateless UDM on data change 17

6 API Definitions 18

6.1 Nudr\_DataRepository Service API 18

6.1.1 API URI 18

6.1.2 Usage of HTTP 18

6.1.2.1 General 18

6.1.2.2 HTTP standard headers 18

6.1.2.2.1 General 18

6.1.2.2.2 Content type 18

6.1.2.2.3 Cache-Control 18

6.1.2.2.4 ETag 18

6.1.2.2.5 If-None-Match 18

6.1.2.2.6 Last-Modified 19

6.1.2.2.7 If-Modified-Since 19

6.1.2.2.8 When to Use Entity-Tags and Last-Modified Dates 19

6.1.2.3 HTTP custom headers 19

6.1.2.3.1 General 19

6.1.2.3.2 3gpp-Sbi-Message-Priority 19

6.1.3 Resources 20

6.1.3.1 Overview 20

6.1.3.2 SubscriptionData 20

6.1.3.3 PolicyData 20

6.1.3.4 StructuredDataForExposure 21

6.1.3.5 ApplicationData 21

6.1.5 Notifications 21

6.1.5.1 General 21

6.1.5.2 Data Change Notification 21

6.1.6 Error Handling 21

6.1.7 Security 22

6.1.8 Feature negotiation 22

Annex A (normative): OpenAPI specification 23

A.1 General 23

A.2 Nudr\_DataRepository API 23

Annex B (informative): Change history 26

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

# 1 Scope

The present document specifies the stage 3 protocol and high level data model for the Nudr Service Based Interface. It provides stage 3 protocol definitions and message flows, and specifies the API for each service offered by the Unified Data Repository (UDR). The data model and usage of the subscription data is specified in 3GPP TS 29.505 [2], and the data model and usage of the policy data, structured data for exposure and application data are specified in 3GPP TS 29.519 [3].

The 5G System architecture is specified in 3GPP TS 23.501 [4]. The stage 2 definition and related procedures for Nudr SBI service are specified in 3GPP TS 23.502 [5] and 3GPP TS 23.503 [6].

The Technical Realization of the Service Based Architecture is specified in 3GPP TS 29.500 [7] and the Principles and Guidelines for Services Definition is specified in 3GPP TS 29.501 [8].

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 29.505: "5G System; Usage of the Unified Data Repository Services for Subscription Data; Stage 3".

[3] 3GPP TS 29.519: "5G System; Usage of the Unified Data Repository Service for Policy Data, Structured Data for Exposure and Application Data; Stage 3".

[4] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[5] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[6] 3GPP TS 23.503: "Policy and Charging Control Framework for the 5G System; Stage 2".

[7] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[8] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[9] IETF RFC 6901(April 2013): "JavaScript Object Notation (JSON) Pointer".

[10] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces Stage 3".

[11] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format".

[12] 3GPP TS 33.501: "Security architecture and procedures for 5G system".

[13] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[14] 3GPP TS 29.510: "Network Function Repository Services; Stage 3".

[15] IETF RFC 7232: "Hypertext Transfer Protocol (HTTP/1.1): Conditional Requests".

[16] IETF RFC 7234: "Hypertext Transfer Protocol (HTTP/1.1): Caching".

# 3 Definitions and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

GPSI Generic Public Subscription Identifier

NEF Network Exposure Function

PCF Policy Control Function

SUPI Subscription Permanent Identifier

UDM Unified Data Management

UDR Unified Data Repository

# 4 Overview

The Unified Data Repository (UDR) is the network entity in the 5G Core Network (5GC) supporting the following functionalities:

- Storage and retrieval of subscription data as specified in 3GPP TS 29.505 [2];

- Storage and retrieval of policy data as specified in 3GPP TS 29.519 [3];

- Storage and retrieval of structured data for exposure as specified in 3GPP TS 29.519 [3];

- Storage and retrieval of application data (including Packet Flow Descriptions (PFDs) for application detection, application request information for multiple UEs) as specified in 3GPP TS 29.519 [3];

- Subscription to notification and the notification of subscribed data changes.

Figures 4-1 shows the data storage architecture for the 5GC:



Figure 4-1: Data storage architecture

The Nudr interface is used by the network functions (i.e. UDM, PCF and NEF) to access a particular set of the data stored in the UDR.

# 5 Services offered by the UDR

## 5.1 Introduction

The UDR offers the following services via the Nudr interface:

- Nudr\_DataRepository Service

NOTE: This service corresponds to the Nudr\_DataManagement service in 3GPP TS 23.501 [4], 3GPP TS 23.502 [5] and 3GPP TS 23.503 [6].

## 5.2 Nudr\_DataRepository Service

### 5.2.1 Service Description

##### 5.2.1.1 Service and operation description

The UDR is acting as NF Service Producer. It provides Unified Data Repository service to the NF service consumer. The NF Service Consumers are the UDM, PCF and NEF.

For the Nudr\_DataRepository service, the following service operations are defined:

- Query

- Create

- Delete

- Update

- Subscribe

- Unsubscribe

- Notify

This service allows NF service consumers to retrieve, create, update, modify and delete data stored in the UDR.

This service allows the NF service consumers to subscribe/unsubscribe the data change notification and to be notified of the data change.

##### 5.2.1.2 Service operation and data access authorization

UDR provides one Nudr\_DataRepository service to all of the NF consumers, while different types of data may have different data access authorizations, the UDR shall be able to have the authorization management mechanism to guarantee the safety of data access.

And the information in the Nudr\_DataRepository service operation should be able to identify the NF type of the consumer and the service operation type or name, and to indicate the requested data information including the data set and data subset, and the resource/data identifier. All HTTP methods for the service operation shall include the information in the appropriate place of the HTTP message.

If there is an illegal service operation or data access request initiated by a NF consumer, the service failure response should be returned through the Nudr interface with an explicit cause value.

### 5.2.2 Service Operations

#### 5.2.2.1 Introduction

This clause specifies the generic Nudr\_DataRepository service operations towards the different data sets as shown in Figure 4-1.

The HTTP request of the service operations contains a resource URI that the {apiSpecificResourceUriPart} (see subclause 4.4.2 in 3GPP TS 29.501[4]) consists of a top-level segment and sub-level segment(s).

For Create, Query, Update and Delete operations, the top-level segment indicates one top level resource representing one of the data sets, which are defined as "/subscription-data", "/policy-data", "/exposure-data" and "/application-data" in Figure 6.1.3.1-1. And a certain child resource is indicated by of the end URI of the sub-level segments, which are defined in 3GPP TS 29.505 [2] for use when the top-level segment is "/subscription-data" and in 3GPP TS 29.519 [3] for use when the top-level segment is "/policy-data", "/exposure-data" or "/application-data".

For Subscribe/Unsubscribe to data change notification operations, the resource of the subscription to the notification should be as the child resource of each of the data sets (i.e. "/subscription-data", "/policy-data", "/exposure-data" and "/application-data"), which are indicated by the top-level segment in the URI. And the resource representation of the subscription to the notification should be indicated by the sub-level segment of each data set.

The following procedures for each operation should be taken as the common procedures and applicable to corresponding detail procedures with the same service operation in 3GPP TS 29.505 [2] and 3GPP TS 29.519 [3].

#### 5.2.2.2 Query

##### 5.2.2.2.1 General

The Query service operation is used to retrieve the data stored in the UDR. HTTP GET method shall be used for the service operation to request the certain data record(s). One piece of data records should be a data set, a data subset, a group of data in one data subset, or a specific data. If the data record(s) are the attribute(s), query parameter or the combination of query parameters should be used as the filters to control the content of result.

##### 5.2.2.2.2 Data retrieval

Figure 5.2.2.2.2-1 shows a scenario where the NF service consumer (e.g. UDM, PCF or NEF) sends a request to the UDR to retrieve data.

Query parameters may be used for data retrieval:

i) Subclause 5.2.2.2.3 specifies the query parameter used for retrieving subset of a resource;

ii) Other query parameters are defined in 3GPP TS 29.505 [2] and 3GPP TS 29.519 [3].



Figure 5.2.2.2.2-1: Retrieving Data

1. The NF service consumer shall send a GET request to the resource representing the data. Query parameters may be used to restrict the response to the requested data record(s) of the resource's representation. Query parameters may also indicate the features that the NF service consumer supports as described in subclause 6.6.2 of 3GPP TS 29.500 [7].

2. On success, the UDR shall respond with "200 OK" with the message body containing the requested data record(s) restricted to the query parameters. (and thus also to the indicated features supported by the NF service consumer).

On failure, the UDR shall return an appropriated error code with the error cause information.

The error codes of corresponding service operations in 3GPP TS 29.505 [2] and 3GPP TS 29.519 [3] shall align and comply with the failure response mechanism which is defined in 3GPP TS 29.500 [7].

##### 5.2.2.2.3 Retrieval of subset of a resource

When a resource has multiple attributes, it is allowed for the NFs to retrieve a subset of the attributes. When the attribute is of type map, it is allowed for the NFs to retrieve individual member(s) of that map. For retrieval of subset of a resource, a new query parameter "fields" is defined to carry the identities of the attributes to be retrieved. The definition of "fields" query parameter is:

1) "fields" query parameter is of type array; and

2) each element of the array is of type string encoded as a JSON pointer as defined IETF RFC 6901 [9].

NOTE: identifying an individual element in the array is supported by JSON pointer, however it is not recommended to use this feature if the client is not exactly aware of the order of the members in the array.

If retrieval of subset of a particular resource is supported, then all the attributes of the corresponding data type of that resource shall be optional or conditional.

EXAMPLE 1:

Given the following representation of ExResource:

{

"lv1Attr1": "value1"

"lv1Attr2": "value2"

"lv1Attr3": {

"lv2Attr1": "value3"

"lv2Attr2": "value4"

}

}

To retrieve "lv1Attr1" and "lv2Attr2", the NF sends the following request:

GET /ExResource?fields=/lv1Attr1, /lv1Attr3/lv2Attr2

Upon success, the UDR then returns the following representation:

{

"lv1Attr1": "value1"

"lv1Attr3": {

"lv2Attr2": "value4"

}

}

EXAMPLE 2:

Given the following representation of ExResource:

{

"Attr1": "value1"

"Attr2": "value2"

"AttrMap": {

"Key1": {ExObject1}

"Key2": {ExObject2}

}

}

To retrieve "Attr1" and the second member of "AttrMap ", the NF sends the following request:

GET /ExResource?fields=/Attr1, /AttrMap/Key2

Upon success, the UDR then returns the following representation:

{

"Attr1": "value1"

"AttrMap": {

"Key2": {ExObject2}

}

}

#### 5.2.2.3 Create

##### 5.2.2.3.1 General

The Create service operation is used by the NF service consumer (e.g. NEF) to create the data into the UDR.

The following procedures using the Create service operation are supported:

- Data creation using PUT

- Data creation using POST

##### 5.2.2.3.2 Data Creation using PUT

Figure 5.2.2.3.2-1 shows a scenario where the NF service consumer (e.g. NEF) sends a request to the UDR to create data. The parent resource of the resource identified by the resource URI shall be of archetype Store (see subclause C.3 in 3GPP TS 29.501[4]).



Figure 5.2.2.3.2-1: Creating Data using PUT

1. The NF service consumer shall send a PUT request to the resource representing the data. The payload body of the PUT request shall contain the representation of the new data.

2. On success, the UDR shall respond with "201 Created" with the payload containing the representation of the created data, and the "Location" header shall be present and contains the URI of the created data.

On failure, the UDR shall return an appropriated error code with the error cause information.

##### 5.2.2.3.3 Data Creation using POST

Figure 5.2.2.3.3-1 shows a scenario where the NF service consumer (e.g. NEF) sends a request to the UDR to create data. The resource identified by the resource URI shall be of archetype Collection (see subclause C.2 in 3GPP TS 29.501[4]).



Figure 5.2.2.3.3-1: Creating Data using POST

1. The NF service consumer shall send a POST request to create the new data record as the child resource of the parent resource in the UDR. The payload body of the POST request shall contain the representation of the new data.

2. The UDR generates the data identifier and constructs the URI for the created data record by appending the data identifier to the parent resource URI received as request URI of the POST request.

On success, the UDR shall respond with "201 Created" with the payload containing the representation of the created data, and the "Location" header shall be present and contains the URI of the created data.

On failure, the UDR shall return an appropriated error code with the error cause information.

#### 5.2.2.4 Delete

##### 5.2.2.4.1 General

The Delete service operation is used by the NF service consumer (e.g. NEF) to remove the data from the UDR.

The following procedures using the Delete service operation are supported:

- Data Deletion

HTTP DELETE method shall be used.

##### 5.2.2.4.2 Deleting Data

Figure 5.2.2.4.2-1 shows a scenario where the NF service consumer (e.g. NEF) sends a request to the UDR to delete a data record.



Figure 5.2.2.4.2-1: Deleting Data

1. The NF service consumer shall send a DELETE request to the resource representing the data. The payload body of the request shall be empty.

2. On success, the UDR shall respond with "204 No Content", the payload body of the DELETE response shall be empty.

On failure, the UDR shall return an appropriated error code with the error cause information.

#### 5.2.2.5 Update

##### 5.2.2.5.1 General

The Update service operation is used by the NF service consumer (e.g. UDM, PCF or NEF) to update the data stored in the UDR.

The following procedures using the Update service operation are supported:

- Data Update using PATCH

- Data Update using PUT

HTTP PATCH method shall be used to add/create, delete or modify part of the value(s) in the data record (e.g. a specific data or a group of data in one data subset). HTTP PUT method shall be used to replace a complete data record.

##### 5.2.2.5.2 Data Update using PATCH

Figure 5.2.2.5.2-1 shows a scenario where the NF service consumer (e.g. UDM, PCF or NEF) sends a request to the UDR to update some parts of the data record.



Figure 5.2.2.5.2-1: Data Updating using PATCH

1. The NF service consumer shall send a PATCH request to the resource representing the data record. The payload body contains the modification instruction towards the data record.

2. On success, the UDR shall respond with "204 No Content".

On failure, the UDR shall return an appropriated error code with the error cause information.

##### 5.2.2.5.3 Data Update using PUT

Figure 5.2.2.5.3-1 shows a scenario where the NF service consumer (e.g. UDM, PCF or NEF) sends a request to the UDR to update the whole data record.



Figure 5.2.2.5.3-1: Data Updating using PUT

1. The NF service consumer shall send a PUT request to the resource representing the data record. The payload body contains the new data for the resource.

2. On success, the UDR shall respond with "204 No Content" or "200 OK".

On failure, the UDR shall return an appropriated error code with the error cause information.

#### 5.2.2.6 Subscribe

##### 5.2.2.6.1 General

The Subscribe service operation is used for the NF service consumer to subscribe to the data change notification from the UDR.

##### 5.2.2.6.2 NF service consumer subscribes to notifications to UDR

Figure 5.2.2.6.2-1 shows a scenario where the NF service consumer (e.g. UDM, PCF or NEF) sends a request to the UDR to subscribe to data change notifications.



Figure 5.2.2.6.2-1: subscribing to data change notifications

1. The NF service consumer sends a POST request to the parent resource (...<top-level segment>/subs-to-notif). The NF service consumer describes the notifications it wants to receive, and it also indicates the features it supports (see subclause 6.6.2 of 3GPP TS 29.500 [7]). The request may contain an expiry time, suggested by the NF Service Consumer as a hint, representing the time upto which the subscription is desired to be kept active.

2. On success, the UDR responds with "201 Created" with the message body containing a representation of the created subscription and indicating the supported features (see subclause 6.6.2 of 3GPP TS 29.500 [7]). The Location HTTP header shall contain the URI of the created subscription. In subsequent notifications according to subclause 5.2.2.8.2, the UDR only uses the indicated supported features.

The response based on operator policies and taking into account the expiry time included in the request, may contain an expiry time (i.e a future timestamp), as determined by the UDR, after which the subscription becomes invalid. If an expiry time was included in the request, then the expiry time returned in the response should be less than or equal to that value. Once the subscription expires, if the NF Service Consumer wants to keep receiving notifications, it shall create a new subscription in the UDR. The UDR shall not provide the same expiry time (i.e a future timestamp) for many subscriptions in order to avoid all of them expiring and recreating the subscription at the same time. If the expiry time is not included in the response, the NF Service Consumer shall consider the subscription to be valid without an expiry time.

On failure, the UDR returns an appropriated error code with the error cause information.

##### 5.2.2.6.3 Stateless UDM subscribes to notifications to UDR

Figure 5.2.2.6.3-1 shows a scenario where the stateless UDM subscribes to notification to the UDR.



Figure 5.2.2.6.3-1: subscribing to data change notifications via stateless UDM

1. The stateless UDM sends a POST request to the UDR to subscribe to the notifications.

The SubData in the POST request body shall indicate the same data for which a change will trigger a notification.

The SubData in the POST request body shall contain a callbackReference URI to which the notifications will be sent to. The host part of the callbackReference URI shall be set to the FQDN of the UDM set to which the stateless UDM belongs.

The SubData in the POST request body shall contain an original callbackReference URI of the NF which initially triggers the subscription.

The request may contain an expiry time, suggested by the NF Service Consumer as a hint, representing the time upto which the subscription is desired to be kept active.

2. On success, the UDR responds with "201 Created" with the message body containing a representation of the created subscription. The Location HTTP header shall contain the URI of the created subscription and that URI shall contain the subscription ID allocated by the UDR.

The response based on operator policies and taking into account the expiry time included in the request, may contain an expiry time (i.e a future timestamp), as determined by the UDR, after which the subscription becomes invalid. If an expiry time was included in the request, then the expiry time returned in the response should be less than or equal to that value. Once the subscription expires, if the NF Service Consumer wants to keep receiving notifications, it shall create a new subscription in the UDR. The UDR shall not provide the same expiry time (i.e a future timestamp) for many subscriptions in order to avoid all of them expiring and recreating the subscription at the same time. If the expiry time is not included in the response, the NF Service Consumer shall consider the subscription to be valid without an expiry time.

On failure, the UDR returns an appropriated error code with the error cause information.

#### 5.2.2.7 Unsubscribe

##### 5.2.2.7.1 General

The Unsubscribe service operation is used for the NF service consumer to unsubscribe to the data change notification from the UDR.

##### 5.2.2.7.2 Unsubscribe service operation

Figure 5.2.2.7.2-1 shows a scenario where the NF service consumer (e.g. UDM, PCF or NEF) sends a request to the UDR to unsubscribe to data change notifications.



Figure 5.2.2.7.2-1: Unsubscribing to the data change notifications

1. The NF service consumer sends a DELETE request to the resource identified by the URI previously received during subscription creation, i.e. in the Location header field of the HTTP 201 Created response.

2. On success, the UDR responds with "204 No Content".

On failure, the UDR returns an appropriated error code with the error cause information.

#### 5.2.2.8 Notify

##### 5.2.2.8.1 General

The Notify service operation is used for the UDR to notify the data change notification to the previous subscribe operation requestor.

##### 5.2.2.8.2 Notification to NF service consumer on data change

Figure 5.2.2.8.2-1 shows a scenario where the UDR notifies the NF service consumer about the subscribed data change. The request contains the CallbackReference URI as previously received in the subscribe operation (see subclause 5.2.2.6).



Figure 5.2.2.8.2-1: Data Change Notification

1. The UDR sends a POST request to the callbackReference URI as provided by the NF service consumer in the subscribe operation.

2. On success, the NF service consumer responds with "204 No Content".  
  
On failure, the NF service consumer responds an appropriated error code with the error cause information.

##### 5.2.2.8.3 Notification to stateless UDM on data change

Figure 5.2.2.8.3-1 shows a scenario where the UDR notifies the NF service consumer about the subscribed data change.



Figure 5.2.2.8.3-1: Data Change Notification to stateless UDM

1. The UDR sends a POST request to the callbackReference URI as provided by the stateless UDM in the subscribe operation.

The notification in the POST request body shall contain the original callbackReference URI which is received in step 1 of Figure 5.2.2.6.3-1.

2. On success, the stateless UDM responds with "204 No Content".

On failure, the stateless UDM responds an appropriated error code with the error cause information.

# 6 API Definitions

## 6.1 Nudr\_DataRepository Service API

### 6.1.1 API URI

URIs of this API shall have the following root:

{apiRoot}/{apiName}/{apiVersion}/

where "apiRoot" is defined in subclause 4.4.1 of 3GPP TS 29.501 [8], the "apiName" shall be set to "nudr-dr" and the "apiVersion" shall be set to "v1" for the current version of this specification.

### 6.1.2 Usage of HTTP

#### 6.1.2.1 General

Nudr service shall comply with the usage of HTTP/2.0 protocol over Service Based Interfaces. (See Clause 5, 3GPP TS 29.500[7]).

#### 6.1.2.2 HTTP standard headers

##### 6.1.2.2.1 General

The usage of HTTP standard headers shall be supported on Nudr interface as defined in subclause 5.2.2 of 3GPP TS 29.500 [7].

##### 6.1.2.2.2 Content type

The JSON format shall be supported for Nudr service. The use of the JSON format (IETF RFC 8259 [11]) shall be signalled by the content type "application/json" or "application/problem+json".

##### 6.1.2.2.3 Cache-Control

As described in IETF RFC 7234 [16] section 5.2, a "Cache-Control" header should be included in HTTP responses carrying a representation of cacheable resources (e.g. SessionManagementSubscriptionData). If it is included, it shall contain a "max-age" value, indicating the amount of time in seconds after which the received response is considered stale.

The "max-age" value shall be configurable by operator policy.

##### 6.1.2.2.4 ETag

As described in IETF RFC 7232 [15] section 2.32, an "ETag" (entity-tag) header should be included in HTTP responses carrying a representation of cacheable resources (e.g. AccessAndMobilitySubscriptionData) to allow an NF Service Consumer performing a conditional request with "If-None-Match" header. If it is included, it shall contain a server-generated strong validator, that allows further matching of this value (included in subsequent client requests) with a given resource representation stored in the server or in a cache.

##### 6.1.2.2.5 If-None-Match

As described in IETF RFC 7232 [15] section 3.2, an NF Service Consumer may issue conditional GET request towards UDR by including an "If-None-Match" header in HTTP requests containing one or several entity tags received in previous responses for the same resource.

##### 6.1.2.2.6 Last-Modified

As described in IETF RFC 7232 [15] section 2.2, a "Last-Modified" header should be included in HTTP responses carrying a representation of cacheable resources (e.g. SmfSelectionSubscriptionData) to allow an NF Service Consumer performing a conditional request with "If-Modified-Since" header.

##### 6.1.2.2.7 If-Modified-Since

As described in IETF RFC 7232 [15] section 3.3, an NF Service Consumer may issue conditional GET request towards UDR, by including an "If-Modified-Since" header in HTTP requests.

##### 6.1.2.2.8 When to Use Entity-Tags and Last-Modified Dates

Both "ETag" and "Last-Modified" headers should be sent in the same HTTP response as stated in IETF RFC 7232 [15] section 2.4.

NOTE: "ETag" is a stronger validator than "Last-Modified" and is preferred.

If the UDR included an "ETag" header with the resource then a conditional request for this resource shall be performed with the "If-None-Match" header.

#### 6.1.2.3 HTTP custom headers

##### 6.1.2.3.1 General

The custom HTTP headers applicable to Nudr service are specified in the following subclauses.

##### 6.1.2.3.2 3gpp-Sbi-Message-Priority

Nudr interface shall support 3gpp-Sbi-Message-Priority custom header. The header contains the HTTP/2 message priority value. See details in Subclause 5.2.3.2.2 of 3GPP TS 29.500 [7].

### 6.1.3 Resources

#### 6.1.3.1 Overview



Figure 6.1.3.1-1: Resource URI structure of the nudr-dr API

Table 6.1.3.1-1 provides an overview of the resources and applicable HTTP methods.

Table 6.1.3.1-1: Resources and methods overview

|  |  |  |  |
| --- | --- | --- | --- |
| Resource name | Resource URI | HTTP method or custom operation | Description |
| SubscriptionData | /subscription-data | none | For sub-level resource names, resource URIs and HTTP methods see 3GPP TS 29.505 [2] |
| PolicyData | /policy-data | none | For sub-level resource names, resource URIs and HTTP methods see 3GPP TS 29.519 [3] |
| StructuredDataForExposure | /exposure-data | none | For sub-level resource names, resource URIs and HTTP methods see 3GPP TS 29.519 [3] |
| ApplicationData | /application-data | none | For sub-level resource names, resource URIs and HTTP methods see 3GPP TS 29.519 [3] |

#### 6.1.3.2 SubscriptionData

See 3GPP TS 29.505 [2].

#### 6.1.3.3 PolicyData

See 3GPP TS 29.519 [3].

#### 6.1.3.4 StructuredDataForExposure

See 3GPP TS 29.519 [3].

#### 6.1.3.5 ApplicationData

See 3GPP TS 29.519 [3].

### 6.1.5 Notifications

#### 6.1.5.1 General

This subclause specifies the general mechanism of notifications of changed data, which are stored in the UDR, and the mechanism should be applicable to the data change notifications, which are specified in 3GPP TS 29.505[2] and 3GPP TS 29.519[3].

#### 6.1.5.2 Data Change Notification

The POST method shall be used for Data Change Notifications and the URI shall be as provided during the subscription procedure.

Resource URI: {callbackReference}

Support of POST request data structures should contain the object of changed data and conditionally the URI of original Callback reference, which is received from the original subscribed NF.

### 6.1.6 Error Handling

Table 6.1.6-1 lists common response body data structures used within the nudr\_dr API

Table 6.1.6-1: Common Response Body Data Structures

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Data type** | **P** | **Cardinality** | **Response**  **codes** | **Description** |
| ProblemDetails | O | 0..1 | 4xx, 5xx responses | For error status codes, the UDR may provide detailed information. |
| NOTE: In addition common data structures as defined in 3GPP TS 29.500 [7] are supported. | | | | |

The "ProblemDetails" data structure may contain a "cause" attribute to indicate the application error, see 3GPP TS 29.571 [10]. The values for "cause" attribute are defined in table 6.1.6-2.

Table 6.1.6-2: Application Errors

|  |  |  |
| --- | --- | --- |
| **Application Error** | HTTP status code | Description |
| NF\_TYPE\_NOT\_ALLOWED | 403 Forbidden | The target data set is not permitted to access for the NF type of the NF consumer. |
| UNSUPPORTED\_MONITORED\_URI | 501 Not Implemented | The subscribe service operation is not able to be implemented due to invalid resource URI to be monitored). |
| USER\_NOT\_FOUND | 404 Not Found | The user indicated in the HTTP/2 request does not exist in the UDR. |
| DATA\_NO\_LONGER\_AVAILABLE | 410 Gone | The data indicated in the HTTP/2 request is no longer available in the UDR. |
| INCORRECT\_CONDITIONAL\_GET\_REQUEST | 412 Precondition Failed | One or more conditions given in the request header fields evaluated to false when tested in the UDR. |
| UNPROCESSABLE\_REQUEST | 422 Unprocessable Entity | The request cannot be procesed due to semantic errors when trying to process a patch method.. |
| DATABASE INCONSISTENCY | 500 Internal Server Error | Requested data cannot be returned due to database inconsistency |
| NOTE: The error codes shall apply to both 3GPP TS 29.505 [2] and 3GPP TS 29.519 [3]. In addition error codes shall comply with the definition in subclause 5.2.7.2 of 3GPP TS 29.500 [7]. | | |

### 6.1.7 Security

As indicated in 3GPP TS 33.501 [12], the access to the Nudr\_DataRepository API may be authorized by means of the OAuth2 protocol (see IETF RFC 6749 [13]), using the "Client Credentials" authorization grant, where the NRF (see 3GPP TS 29.510 [14]) plays the role of the authorization server.

If Oauth2 authorization is used, an NF Service Consumer, prior to consuming services offered by the Nudr\_DataRepository API, shall obtain a "token" from the authorization server, by invoking the Access Token Request service, as described in 3GPP TS 29.510 [14], subclause 5.4.2.2.

NOTE: When multiple NRFs are deployed in a network, the NRF used as authorization server is the same NRF that the NF Service Consumer used for discovering the Nudr\_DataRepository service.

The Nudr\_DataRepository API defines scopes for OAuth2 authorization as specified in 3GPP TS 33.501 [12]; it defines a single scope consisting on the name of the service (i.e., "nudr-dr"), and it does not define any additional scopes at resource or operation level.

### 6.1.8 Feature negotiation

The optional features in table 6.1.8-1 are defined for the Nudr\_DataRepository API. They shall be negotiated using the extensibility mechanism defined in subclause 6.6 of 3GPP TS 29.500 [7].

Table 6.1.8-1: Supported Features

|  |  |  |
| --- | --- | --- |
| **Feature number** | **Feature Name** | **Description** |
|  |  |  |

Annex A (normative):  
OpenAPI specification

## A.1 General

This document specifies the common service operations and the top level data model for Nudr\_DataRepository Service Based Interface. There are no specific HTTP methods or custom operations on the four top level resources in Table 6.1.3.1-1. Hence, the top level OpenAPI specification is not needed.

## A.2 Nudr\_DataRepository API

This Annex specifies the formal definition of the Nudr\_DataRepository service. It consists of OpenAPI 3.0.0 specifications, in YAML format.

The OpenAPI 3.0.0 definition related to SubscriptionData shall comply with the definition in 3GPP TS 29.505 [2].

The OpenAPI 3.0.0 definition related to PolicyData, StructuredDataForExposure and ApplicationData shall comply with the definition in 3GPP TS 29.519 [3].

The OpenAPI file for the Nudr\_DataRepository API is defined as follows:

openapi: 3.0.0

info:

version: 1.0.0

title: 'Nudr\_DataRepository API OpenAPI file'

description: 'Unified Data Repository Service'

externalDocs:

description: 3GPP TS 29.504 V15.2.0; 5G System; Unified Data Repository Services; Stage 3

url: 'http://www.3gpp.org/ftp/Specs/archive/29\_series/29.504/'

servers:

- description: API root

url: '{apiRoot}/nudr-dr/v1'

variables:

apiRoot:

default: https://example.com

security:

- {}

- oAuth2ClientCredentials:

- nudr-dr

paths:

/subscription-data/{ueId}/authentication-data:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1authentication-data'

/subscription-data/{ueId}/{servingPlmnId}/provisioned-data/am-data:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1%7BservingPlmnId%7D~1provisioned-data~1am-data'

/subscription-data/{ueId}/{servingPlmnId}/provisioned-data/smf-selection-subscription-data:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1%7BservingPlmnId%7D~1provisioned-data~1smf-selection-subscription-data'

/subscription-data/{ueId}/{servingPlmnId}/provisioned-data/sm-data:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1%7BservingPlmnId%7D~1provisioned-data~1sm-data'

/subscription-data/{ueId}/context-data/amf-3gpp-access:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1context-data~1amf-3gpp-access'

/subscription-data/{ueId}/context-data/amf-non-3gpp-access:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1context-data~1amf-non-3gpp-access'

/subscription-data/{ueId}/context-data/smf-registrations:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1context-data~1smf-registrations'

/subscription-data/{ueId}/context-data/smf-registrations/{pduSessionId}:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1context-data~1smf-registrations~1%7BpduSessionId%7D'

/subscription-data/{ueId}/operator-specific-data:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1operator-specific-data'

/subscription-data/{ueId}/context-data/smsf-3gpp-access:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1context-data~1smsf-3gpp-access'

/subscription-data/{ueId}/context-data/smsf-non-3gpp-access:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1context-data~1smsf-non-3gpp-access'

/subscription-data/{ueId}/{servingPlmnId}/provisioned-data/sms-mng-data:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1%7BservingPlmnId%7D~1provisioned-data~1sms-mng-data'

/subscription-data/{ueId}/{servingPlmnId}/provisioned-data/sms-data:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1%7BservingPlmnId%7D~1provisioned-data~1sms-data'

/subscription-data/{ueId}/pp-data:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1pp-data'

/subscription-data/{ueId}/context-data/ee-subscriptions:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1context-data~1ee-subscriptions'

/subscription-data/{ueId}/context-data/ee-subscriptions/{subsId}:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1context-data~1ee-subscriptions~1%7BsubsId%7D'

/subscription-data/{ueId}/context-data/sdm-subscriptions:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1context-data~1sdm-subscriptions'

/subscription-data/{ueId}/context-data/sdm-subscriptions/{subsId}:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1context-data~1sdm-subscriptions~1%7BsubsId%7D'

/subscription-data/subs-to-notify:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1subs-to-notify'

/subscription-data/subs-to-notify/{subsId}:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1subs-to-notify~1%7BsubsId%7D'

/subscription-data/{ueId}/{servingPlmnId}/provisioned-data/trace-data:

$ref: 'TS29505\_Subscription\_Data.yaml#/paths/~1subscription-data~1%7BueId%7D~1%7BservingPlmnId%7D~1provisioned-data~1trace-data'

/policy-data/{ueId}/am-data:

$ref: 'TS29519\_Policy\_Data.yaml#/paths/~1policy-data~1%7BueId%7D~1am-data'

/policy-data/{ueId}/ue-policy-set:

$ref: 'TS29519\_Policy\_Data.yaml#/paths/~1policy-data~1%7BueId%7D~1ue-policy-set'

/policy-data/{ueId}/sm-data:

$ref: 'TS29519\_Policy\_Data.yaml#/paths/~1policy-data~1%7BueId%7D~1sm-data'

/policy-data/{ueId}/sm-data/{usageMonId}:

$ref: 'TS29519\_Policy\_Data.yaml#/paths/~1policy-data~1%7BueId%7D~1sm-data~1%7BusageMonId%7D'

/policy-data/sponsor-connectivity-data/{sponsorId}:

$ref: 'TS29519\_Policy\_Data.yaml#/paths/~1policy-data~1sponsor-connectivity-data~1%7BsponsorId%7D'

/policy-data/bdt-data:

$ref: 'TS29519\_Policy\_Data.yaml#/paths/~1policy-data~1bdt-data'

/policy-data/bdt-data/{bdtReferenceId}:

$ref: 'TS29519\_Policy\_Data.yaml#/paths/~1policy-data~1bdt-data~1%7BbdtReferenceId%7D'

/policy-data/subs-to-notify:

$ref: 'TS29519\_Policy\_Data.yaml#/paths/~1policy-data~1subs-to-notify'

/policy-data/subs-to-notify/{subsId}:

$ref: 'TS29519\_Policy\_Data.yaml#/paths/~1policy-data~1subs-to-notify~1%7BsubsId%7D'

/policy-data/{ueId}/operator-specific-data:

$ref: 'TS29519\_Policy\_Data.yaml#/paths/~1policy-data~1%7BueId%7D~1operator-specific-data'

/application-data/pfds:

$ref: 'TS29519\_Application\_Data.yaml#/paths/~1application-data~1pfds'

/application-data/pfds/{application-identifier}:

$ref: 'TS29519\_Application\_Data.yaml#/paths/~1application-data~1pfds~1%7Bapplication-identifier%7D'

/application-data/influenceData:

$ref: 'TS29519\_Application\_Data.yaml#/paths/~1application-data~1influenceData'

/application-data/influenceData/{afServiceId}:

$ref: 'TS29519\_Application\_Data.yaml#/paths/~1application-data~1influenceData~1%7BafServiceId%7D'

/application-data/influenceData/subscriptions:

$ref: 'TS29519\_Application\_Data.yaml#/paths/~1application-data~1influenceData~1subscriptions'

/application-data/influenceData/subscriptions/{subscriptionId}:

$ref: 'TS29519\_Application\_Data.yaml#/paths/~1application-data~1influenceData~1subscriptions~1%7BsubscriptionId%7D'

/exposure-data/{ueId}/access-and-mobility-data:

$ref: 'TS29519\_Exposure\_Data.yaml#/paths/~1exposure-data~1%7BueId%7D~1access-and-mobility-data'

/exposure-data/{ueId}/session-management-data:

$ref: 'TS29519\_Exposure\_Data.yaml#/paths/~1exposure-data~1%7BueId%7D~1session-management-data'

/exposure-data/{ueId}/session-management-data/{pduSessionId}:

$ref: 'TS29519\_Exposure\_Data.yaml#/paths/~1exposure-data~1%7BueId%7D~1session-management-data~1%7BpduSessionId%7D'

/exposure-data/subs-to-notify:

$ref: 'TS29519\_Exposure\_Data.yaml#/paths/~1exposure-data~1subs-to-notify'

/exposure-data/subs-to-notify/{subId}:

$ref: 'TS29519\_Exposure\_Data.yaml#/paths/~1exposure-data~1subs-to-notify~1%7BsubId%7D'

components:

securitySchemes:

oAuth2ClientCredentials:

type: oauth2

flows:

clientCredentials:

tokenUrl: '{nrfApiRoot}/oauth2/token'

scopes:

nudr-dr: Access to the Nudr\_DataRepository API

Annex B (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2018-01 | CT4#82 | C4-181365 |  |  |  | TS skeleton | 0.0.0 |
| 2018-01 | CT4#82 | C4-181396 |  |  |  | Inclusion of pCRs agreed at CT4#82, including C4-181366, C4-181367, C4-181323 and C4-181385. | 0.1.0 |
| 2018-03 | CT4#83 | C4-182441 |  |  |  | Inclusion of pCRs agreed at CT4#83, including C4-182337, C4-182429. | 0.2.0 |
| 2018-04 | CT4#84 | C4-183522 |  |  |  | Inclusion of pCRs agreed at CT4#84, including C4-183497, C4-183295, C4-183296, C4-183297, C4-183102, C4-183420, C4-183498. | 0.3.0 |
| 2018-05 | CT4#85 | C4-184636 |  |  |  | Inclusion of pCRs agreed at CT4#85, including C4-184482, C4-184484, C4-184167, C4-184168, C4-184489, C4-184564, C4-184637. | 0.4.0 |
| 2018-06 | CT#80 | CP-181102 |  |  |  | Presented for information and approval | 1.0.0 |
| 2018-06 | CT#80 |  |  |  |  | Approved in CT#80. | 15.0.0 |
| 2018-09 | CT#81 | CP-182057 | 0002 | 1 | F | Service Name | 15.1.0 |
| 2018-09 | CT#81 | CP-182057 | 0006 | 2 | F | Supported Features Negotiation | 15.1.0 |
| 2018-09 | CT#81 | CP-182057 | 0004 | 2 | F | Error handling in UDR | 15.1.0 |
| 2018-09 | CT#81 | CP-182211 | 0003 | 4 |  | OpenAPI file for Nudr\_DataRepository API | 15.1.0 |
| 2018-10 | CT#82 | CP-183015 | 0008 |  | F | Update the Reference point name | 15.2.0 |
| 2018-10 | CT#82 | CP-183015 | 0009 |  | F | Introduction of Barring of Roaming in 5GC | 15.2.0 |
| 2018-10 | CT#82 | CP-183015 | 0010 | 1 | F | Shared Data | 15.2.0 |
| 2018-10 | CT#82 | CP-183015 | 0011 |  |  | Get multiple datasets for ProvsionedData | 15.2.0 |
| 2018-10 | CT#82 | CP-183015 | 0012 | 1 | F | Definition of Authentication Data | 15.2.0 |
| 2018-12 | CT#82 | CP-183015 | 0013 | 1 | F | Adding headers for cache control and conditional request to the Nudr Services API | 15.2.0 |
| 2018-12 | CT#82 | CP-183015 | 0014 |  |  | APIRoot Clarification | 15.2.0 |
| 2018-12 | CT#82 | CP-183015 | 0015 | 2 | F | lifetime of subscription | 15.2.0 |
| 2018-12 | CT#82 | CP-183015 | 0016 | 1 | F | Authorized Event Types | 15.2.0 |
| 2018-12 | CT#82 | CP-183015 | 0017 |  |  | Group Subscription Path | 15.2.0 |
| 2018-12 | CT#82 | CP-183177 | 0018 | 2 | F | PLMN ID as key for UE data sets | 15.2.0 |
| 2018-12 | CT#82 | CP-183241 | 0020 | 1 | F | Correction to Nudr\_DataRepository service OpenAPI | 15.2.0 |